{"text_format":"1","workbook":"xlsx","n_sheets":6,"sheets":["official channels","lower Channels","lower B channels","upper D channels","upper E channels","Feuil1"],"not_rendered":{"charts":0,"images":2,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"official channels","index":0,"n_rows":22,"n_cols":4,"rows_kept":22,"cut":false,"hidden":false,"merged":[[0,0,0,3]]}
["Cannaux Officiels"]
["Channel","FREQUENCY (MHz)","Channel2","FREQUENCY (MHz)2"]
["1-OC",26.965,"21-OC",27.215]
["2-OC",26.975000000000001,"22-OC",27.225000000000001]
["3-OC",26.984999999999999,"23-OC",27.254999999999999]
["4-OC",27.004999999999999,"24-OC",27.234999999999999]
["5-OC",27.015000000000001,"25-OC",27.245000000000001]
["6-OC",27.024999999999999,"26-OC",27.265000000000001]
["7-OC",27.035,"27-OC",27.274999999999999]
["8-OC",27.055,"28-OC",27.285]
["9-OC",27.065000000000001,"29-OC",27.295000000000002]
["10-OC",27.074999999999999,"30-OC",27.305]
["11-OC",27.085000000000001,"31-OC",27.315000000000001]
["12-OC",27.105,"32-OC",27.324999999999999]
["13-OC",27.114999999999998,"33-OC",27.335000000000001]
["14-OC",27.125,"34-OC",27.344999999999999]
["15-OC",27.135000000000002,"35-OC",27.355]
["16-OC",27.155000000000001,"36-OC",27.364999999999998]
["17-OC",27.164999999999999,"37-OC",27.375]
["18-OC",27.175000000000001,"38-OC",27.385000000000002]
["19-OC",27.184999999999999,"39-OC",27.395]
["20-OC",27.204999999999998,"40-OC",27.405000000000001]

{"sheet":"lower Channels","index":1,"n_rows":22,"n_cols":4,"rows_kept":22,"cut":false,"hidden":false,"merged":[[0,0,0,3]]}
["Canaux inférieurs A"]
["Channel","Fréquency(MHz)","Channel2","Fréquency (MHz)2"]
["1-IA",26.065000000000001,"21-IA",26.315000000000001]
["2-IA",26.074999999999999,"22-IA",26.324999999999999]
["3-IA",26.085000000000001,"23-IA",26.355]
["4-IA",26.105,"24-IA",26.335000000000001]
["5-IA",26.114999999999998,"25-IA",26.344999999999999]
["6-IA",26.125,"26-IA",26.364999999999998]
["7-IA",26.135000000000002,"27-IA",26.375]
["8-IA",26.155000000000001,"28-IA",26.385000000000002]
["9-IA",26.164999999999999,"29-IA",26.395]
["10-IA",26.175000000000001,"30-IA",26.405000000000001]
["11-IA",26.184999999999999,"31-IA",26.414999999999999]
["12-IA",26.204999999999998,"32-IA",26.425000000000001]
["13-IA",26.215,"33-IA",26.434999999999999]
["14-IA",26.254999999999999,"34-IA",26.445]
["15-IA",26.234999999999999,"35-IA",26.454999999999998]
["16-IA",26.254999999999999,"36-IA",26.465]
["17-IA",26.265000000000001,"37-IA",26.475000000000001]
["18-IA",26.274999999999999,"38-IA",26.484999999999999]
["19-IA",26.285,"39-IA",26.495000000000001]
["20-IA",26.305,"40-IA",26.504999999999999]

{"sheet":"lower B channels","index":2,"n_rows":22,"n_cols":5,"rows_kept":22,"cut":false,"hidden":false,"merged":[[0,0,0,3]]}
["Canaux inférieurs B"]
["Channel","Fréquency (MHz)","Channel2","Fréquency (MHz)2","Fréquency (MHz)3"]
["1-IB",26.515000000000001,"21-IB",26.765000000000001]
["2-IB",26.524999999999999,"22-IB",26.774999999999999]
["3-IB",26.535,"23-IB",26.785]
["4-IB",26.555,"24-IB",26.795000000000002]
["5-IB",26.565000000000001,"25-IB",26.805]
["6-IB",26.574999999999999,"26-IB",26.815000000000001]
["7-IB",26.585000000000001,"27-IB",26.824999999999999]
["8-IB",26.605,"28-IB",26.835000000000001]
["9-IB",26.515000000000001,"29-IB",26.844999999999999]
["10-IB",26.625,"30-IB",26.855]
["11-IB",26.635000000000002,"31-IB",26.864999999999998]
["12-IB",26.655000000000001,"32-IB",26.875]
["13-IB",26.664999999999999,"33-IB",26.885000000000002]
["14-IB",26.675000000000001,"34-IB",26.895]
["15-IB",26.684999999999999,"35-IB",26.905000000000001]
["16-IB",26.704999999999998,"36-IB",26.914999999999999]
["17-IB",26.715,"37-IB",26.925000000000001]
["18-IB",26.725000000000001,"38-IB",26.934999999999999]
["19-IB",26.734999999999999,"39-IB",26.945]
["20-IB",26.754999999999999,"40-IB",26.954999999999998]

{"sheet":"upper D channels","index":3,"n_rows":22,"n_cols":4,"rows_kept":22,"cut":false,"hidden":false,"merged":[[0,0,0,3]]}
["Canaux supérieurs  D"]
["Channel","Fréquency (MHz)","Channel2","Fréquency (MHz)2"]
["1-SD",27.414999999999999,"21-SD",27.664999999999999]
["2-SD",27.425000000000001,"22-SD",27.675000000000001]
["3-SD",27.434999999999999,"23-SD",27.704999999999998]
["4-SD",27.454999999999998,"24-SD",27.684999999999999]
["5-SD",27.465,"25-SD",27.695]
["6-SD",27.475000000000001,"26-SD",27.715]
["7-SD",27.484999999999999,"27-SD",27.725000000000001]
["8-SD",27.504999999999999,"28-SD",27.734999999999999]
["9-SD",27.515000000000001,"29-SD",27.745000000000001]
["10-SD",27.524999999999999,"30-SD",27.754999999999999]
["11-SD",27.535,"31-SD",27.765000000000001]
["12-SD",27.555,"32-SD",27.774999999999999]
["13-SD",27.565000000000001,"33-SD",27.785]
["14-SD",27.574999999999999,"34-SD",27.795000000000002]
["15-SD",27.585000000000001,"35-SD",27.805]
["16-SD",27.605,"36-SD",27.815000000000001]
["17-SD",27.614999999999998,"37-SD",27.824999999999999]
["18-SD",27.625,"38-SD",27.835000000000001]
["19-SD",27.635000000000002,"39-SD",27.844999999999999]
["20-SD",27.655000000000001,"40-SD",27.855]

{"sheet":"upper E channels","index":4,"n_rows":13,"n_cols":4,"rows_kept":13,"cut":false,"hidden":false,"merged":[[0,0,0,3]]}
["Canaux Supérieurs E"]
["Channel","Fréquency (MHz)","Channel2","Fréquency(MHz)2"]
["1-SE",27.864999999999998]
["2-SE",27.675000000000001]
["3-SE",27.885000000000002]
["4-SE",27.905000000000001]
["5-SE",27.914999999999999]
["6-SE",27.925000000000001]
["7-SE",27.934999999999999]
["8-SE",27.954999999999998]
["9-SE",27.965]
["10-SE",27.975000000000001]
["11-SE",27.984999999999999]

{"sheet":"Feuil1","index":5,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}